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[bookmark: _Hlk168907479]Replacing dilapidated picket Fence on West elevation

The existing timber picket fence is in a poor state of repair. We are continuously carrying out repairs and replacing rotton posts. Further damage has occurred during the recent storms

Existing fence
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Proposed Replacement Fence
The proposal would be to replace the fence with a metal Estate style fence with uprights at maximum 1m centres and 5no horizontal rails following the contours of the existing boundary line
The proposed uprights will be as style F3
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There will be 60mmx60mmx4mm SHS steel strengthening posts in locations shown on the proposed elevation drawing no. 1306 & the tops will be complete with Urns as shown below
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The photo below shows a similar fence 
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The new steel estate fence will be finished in RAL7033 colour paint, the same as the existing entrance gates and the house windows.
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