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Proposal

To add a two storey extension to the rear of the house. Also to provide a new driveway from the main road that will require a bridge over a small waterway.
The Site
The site is flat to gently inclining towards the south at 55.5m above average sea level. The site is shown to be in a Flood Zone 2 & Flood Zone 3.
Environment Agency Flood Map
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Flood Zones 2 & 3
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Defence Information
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100 year JFLOW fluvial water depths.
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377362-WX - JFLOW Fiuvial Water depths (m) Without Flood Defences. 100 year (1% AEP) centred on land at Devizes (396599, 156752).
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1000 year JFLOW fluvial water depths.
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Long term flooding risk to the development

From data received from the Environment Agency, both the 100 year & 1000 year prediction shows potential flooding to the west & south of the house but further down the garden. The risk of flooding is low at 1% or less for 100 years and 0.1% or less for 1000 years. The applicant is not aware of the property having a history of flooding.
Top of Form

Design against flood.
As part of the build it is intended to incorporate flood protection with the new floor being the same level as the existing or possibly higher. All ground floor floors will be of concrete. Doors to incorporate flood board guides.

Similar precautions were accepted with nearby application 13/01656/FUL 
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