Proposed new dwelling at 28 Horsepool Bromham – Block 9 Developments limited
Bat box, Bird box and Bee brick information sheet.
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Home > Segovia Build-in WoodStone Bat Box

SEGOVIA BUILD-IN WOODSTONE BAT
BOX

SKU 11349

£35.50: ® 127 I Stock For Immediate Dispatch.

Quantity 1
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There are various bat species that can use the Segovia bat box, this depends on the species that occur locally and where
the bat box is located. The box will be used during the summer and in mild winters for roosting and shelter.

‘The Woodstone material offers good thermal insulation and therefore creates a more stable internal temperature and
rough surface to ensure bats have enough grip to access the box. In addition to creating optimal conditions within the box,
Woodstone habitats also help protect inhabitants from predators.

The installation block for bats can be integrated into new buildings or building renovations. It can be flush with the facade
or be slightly recessed in the facade. When installing in the cavity wall, the thermal insulation runs behind the stone, so
there is no cold bridge. The building blocks can also be connected to one another. To do this, remove the wooden element
on the left or right. This allows the bats to crawl from one stone to the next. Basically, this creates alarge bat box in the
cavity wall.

Either side of the house is suitable for installation, but the south side is preferable. Mount the module as high as possible,
but at least 2.5m high. Keep the approach route to the box clear, ie. do not plant trees or bushes in front of the wall in
question and do not mount an awning or the like over the installation block.

Thanks to the sloping bottom of the built-in block, the bat droppings roll out of the box. Otherwise this module is also
maintenance-free.

Dimensions:
Bottom secti
Top section: 50cm x 21cm x 5cm
Conforms with UK brick sizes

: 14cm x 21cm x 15cm
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Home > Woodstone Build-In Swift Box Visible - UK Brick Size:

WOODSTONE BUILD-IN SWIFT BOX
VISIBLE - UK BRICK SIZE

SKU 10746

£39.40% ® 67 In Stock For Immediate Dispatch.

Quantity 1
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Introducing our brand-new Swift Box, tailor-made to British brick size standards. This ‘it & forget" nest box is perfect for
incorporation into new builds or renovations, especially in those elusive spots swifts favour, such as beneath the eaves.
Like every product in our WoodStone® range, this nest box guarantees its residents safety from potential predators and

insulation against temperature fluctuations.

SITING

‘This Swift building block is suitable for both new constructions and renovations. It's crafted to integrate seamlessly into a
wall. The block aligns with the front wall, protruding roughly 50mm into the cavity, whilst leaving an additional 50mm or
beyond for insulation when positioned against a heated space. Internally, it boasts two nesting compartments, permitting
the box to be affixed with the entrance to the left or right, as per your liking.

in the cavity can effortlessly extend behind the block, thereby preventing a thermal bridge. If insulation
needs trimming, ensure itis sculpted around the block's perimeter.

The block is also compatible with a rendered wall due to its flat WoodStone front. During application, utilise a former to

safeguard the entrance hole from becoming obstructed or diminishing in size.

Ideally, mount the in-built block on the north or east gable end, approximately three courses below the apex. This
establishes the optimal elevation for the block in a region with minimal human interference. Maintain a clear flight
trajectory for the nesting box by preventing trees or shrubs from sprouting directly in front of the wall. Given swifts'
penchant for breeding in colonies, it's prudent to install multiple building blocks in proximity. Ensure a minimum gap of 40
centimetres between each block. There's no need to supply any nesting materials. For best results, we advise placing at
least one block for each new residence. For instance, a 30-home development would ideally feature 30 blocks.
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Home > GreenaBlu Bee Brick
GREEN&BLUE BEE BRICK
'SKU BEE BRICK.
£31.66% © 152 In Stock For Immediate Dispatch.
Colour Red (£31.66) (In stock) A
Quantity 1
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Bee Brick® solitary bee houses designed and made by Green&Blue in the UK.

Materials Made fom concrete, using up to 75% recycled material from the Cornish China clay industry.

Dimensions 215mm x 105mm x 65mm

Weight 2.9 kg (unpackaged)

Positioning The Bee Brick® should be positioned in awarm sunny spot, south facing, with no vegetation in front of the
fascia. Ideally placed at least 1 metre from the ground with no upward limit.

Bee Brick® s solid at the back and has moulded cavities where the bees will lay their eggs, sealing the entrance with mud
or chewed up vegetation. Offspring emerge in the Spring and begin the process of nesting again, repeating the cycle.




