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Windows and Doors

The majority of the existing windows and doors at Bennells are beyond repair, many have had repair works carried out previously and we would now wish to replace them with new windows and doors. The existing are single glazed and condensate internally. 

Bennells is in a conservation area and we propose to replace the existing with windows and doors to closely match existing.
Planning Approval was granted on application ref PL/2034/05543

The existing Windows and Door frames are in Sapele hardwood and softwood. The proposal is to replace them using French Oak, deliberately cosmetically aged with dye and natural finish. Handpicked Grade A Oak from  specific Oak Supplier Hewins . 
We propose to use 9 mm single acoustic glass toughened to Building Control requirements where necessary, 21 mm structural glazing bars cut in fine lambs tongue beaded in oak to glass. 
Glass to have only a small furniture stamp of Pilkingtons’.
Doors 58 mm thick Oak with glazing bars same as windows, toughened glass to accord with building regs. All frames thresholds weather boards drip strips  all in cosmetically aged Oak .
[bookmark: _Hlk168907479]















East Elevation
[bookmark: _Hlk168907843][image: A bench in front of a brick building

Description automatically generated][image: A door to a brick building

Description automatically generated]Kitchen Ground Floor – Window W1 and Door D1
[bookmark: _Hlk198815185]Master Bedroom First Floor – 2 windows - W2 and W3 are habitable rooms 
[image: A brick building with windows

Description automatically generated]and they must have an unobstructed opening of 0.33m², with a minimum clear opening width of at least 450mm
[image: A brick building with windows

Description automatically generated]
[image: A brick building with windows

Description automatically generated][image: A white door with glass panes

Description automatically generated]Kitchen No 2 Ground Floor                          Kitchen No 2 Ground Floor 
Window W4                                                  Door D2

[image: A brick building with a window

Description automatically generated]Bathroom No 2 Ground Floor     			Landing First Floor - 
Window W5						Window W6
[image: A window with white curtains

Description automatically generated] 
North Elevation
[bookmark: _Hlk168908185][bookmark: _Hlk168907994][bookmark: _Hlk168908192][image: A window in a brick wall

Description automatically generated]Kitchen Ground Floor                      			Hall Ground Floor
Window W7 						Window W8 
[image: A window on a brick building

Description automatically generated]
[image: A brick house with a door and a wreath

Description automatically generated]Hall Ground Floor                                        		Landing First Floor – 
Door D3							Window W9
[image: A brick house with a door and a wreath

Description automatically generated]
Drawing Room Ground Floor                			Bath & Bed First F[image: A brick building with a window

Description automatically generated][image: A brick building with a window

Description automatically generated]loor
Window W10							Windows W11 & W12          
W11 and W12 is to the same habitable room and one window must have an unobstructed opening of 0.33m², with a minimum clear opening width of at least 450mm
[bookmark: _Hlk168909948]

















West Elevation
[image: A brick building with a window

Description automatically generated][image: A window in a brick building

Description automatically generated][image: A window in a brick building

Description automatically generated]Drawing Room Ground Floor - 3 no Windows W13, W14 & W15                           

Lounge 2 Ground Floor – 2no Windows W16 & W17                           
[image: A window in a brick building

Description automatically generated][image: A window in a brick building

Description automatically generated]


[image: A window in a brick building

Description automatically generated]Kitchen No 2 Ground Floor – Window W18

Guest Bedrooms First Floor – 2no Windows W19 & W20   
W19 and W20 are habitable rooms and they must have an unobstructed opening of 0.33m², with a minimum clear opening width of at least 450mm
[image: A brick house with a chimney

Description automatically generated][image: A brick house with windows

Description automatically generated]
South Elevation
[image: A window with a white frame

Description automatically generated with medium confidence]Kitchen No 2 Ground Floor       			Kitchen Alley Ground Floor 
[image: A window with a white frame

Description automatically generated]Window W21						Window W22


[image: A brick building with a window

Description automatically generated]En Suite Alley – First Floor Window W23 

Spare Bedrooms First Floor – 2no Windows W24 & W25 

W24 and W25 are habitable rooms and they must have an unobstructed opening of 0.33m², with a minimum clear opening width of at least 450mm
[image: A brick building with a window

Description automatically generated][image: A brick building with a window
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