Method Statement for the Creation of the Ground Floor East Window

The new ground floor window will be formed with hand tools wherever possible. An initial hole in the centre of the opening will required machine drilling, but beyond this it should be possible to tool the stonework working outwards by hand to reach the desired opening size. Larger overlapping stones will not be removed and reset to create the opening. It is hoped that no new mortar will be required, but any needed will match in colour, texture and composition (lime) to that already in situ.

