SITE LAYOUT PLAN DESCRIPTION
Proposed Development: Padel Courts (2 no.)
Location: Fairfields, Semington, Trowbridge, BA14 6JD

1. Overview
This document describes the proposed site layout for the development of two padel courts and associated facilities on land at Fairfields.
The layout has been designed to maximise efficient use of space while maintaining appropriate separation from site boundaries and neighbouring properties, and minimising environmental and visual impact.

2. Access and Arrival
Access to the site is taken from the A361 via an existing site entrance.
· The track extends approximately 40 metres to the development area
· No alterations to the existing access are proposed
· Vehicles will arrive and proceed directly to the designated parking area

3. Parking Area
A small parking area is located within the site to serve the facility:
· Capacity for approximately 6–8 vehicles
· Positioned to the rear of the welfare building (portacabin)
· Designed to allow safe manoeuvring and turning within the site
· Finished in a permeable or low-impact surface where possible

4. Welfare Facilities
A portacabin unit is located between the parking area and the courts:
· Provides toilet and hand-washing facilities
· Positioned for convenient access by users
· Connected to:
· Water supply from existing line along front hedge
· Septic tank located at lower end of the field

5. Decking / Waiting Area
A small timber decking area is located adjacent to the courts:
· Acts as a waiting and viewing space
· Positioned to provide clear visibility of both courts
· Designed to be low-profile and visually unobtrusive

6. Padel Courts Layout
The main development comprises:
· 2 no. padel courts, each measuring 20m x 10m x 4m high
· Courts arranged side by side
Spacing includes:
· 2 metres between the courts
· 2 metres clearance at each end
This layout ensures:
· Safe circulation around courts
· Adequate maintenance access
· Compliance with typical operational standards

7. Construction Approach
The courts will be installed using an iframe modular system, consisting of:
· A steel ring beam foundation system
· No requirement for traditional concrete slab or extensive excavation
· Reduced ground disturbance and improved reversibility
The playing surface will be contained within the structure without large-scale permanent surfacing works.

8. Lighting Arrangement
Each court will be served by:
· 4 no. LED lighting columns (8 total)
· Mounted at approximately 6 metres height
· Positioned at court corners or sides
Lighting is:
· Directional and downward facing
· Designed to minimise spill beyond the courts

9. Drainage and Services
· Water supply taken from existing service along the front hedge line
· Foul drainage directed to a septic tank located at the lower end of the field
· Surface water will naturally drain within the grassed site with minimal impermeable surfacing introduced

10. Relationship to Surroundings
· The nearest residential properties are approximately 25 metres from the rear of the courts
· The development is positioned to centralise activity within the site
· Existing boundaries and vegetation help provide natural screening

11. Summary
The layout has been carefully designed to:
· Provide a functional and efficient sports facility
· Minimise environmental and visual impact
· Maintain safe access and circulation
· Protect neighbouring amenity
The proposal represents a well-considered and low-impact use of the site, appropriate to its rural context.
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