Mr & Mrs Townley-Berry
The Old Manor House
Church Road
Milston
Salisbury
SP4 8HT 
										10th April 2026

Ref: Heritage Design and Access Statement Application for listed building consent - PL/2026/01955

What should be included in a Design and Access Statement accompanying an application for listed building consent
1. Design and Access Statements accompanying applications for listed building consent must include an explanation of the design principles and concepts that have been applied to the proposed works, and how they have taken account of:
(a) the special architectural or historic importance of the building;

I. The Old Manor House is a detached Grade II* listed property dating back to 1632 with distinctive flint elevations, stone mullion windows, tall gables and a steeply pitched roof. The property has a Jacobean staircase across the three floors. 
 
My parents are elderly and need access to the top floor, however, we did not want to make any changes to the original staircase, which is difficult to ascend, given their age, and is particularly steep. 

To facilitate access to the top floor we removed a small corner section of the ceiling and installed a staircase with two handrails, one each side to provide access and reduce the risk of falling.  This has had no impact on significance of the building.

II. The works completed only affect the interior of the building, nevertheless, great care has been taken to ensure that appropriate design principles and concepts have been applied, whilst ensuring that materials and workmanship comply in all respects with current British Standard specifications, Codes of Practice, and Building Regulations. 
 
III.  All open section steelwork (UB, UC etc.) is graded S355jr fabricated, primed and installed in accordance with BS5950 & EN10025-2. 

IV. All closed sections steelwork (RHS, SHS etc.) is graded S355j2h fabricated, primed and installed in accordance with BS5950 & EN10210.  

V. All fixtures and fittings are graded S275. 

VI. All steelwork is in accordance with National Structural Steel Specification (N.S.S.S.) and all steelwork and components were manufactured in accordance with execution class EXC2 to BS EN1090-2. 

VII. All welds are metal arc 6mm full profile fillet welds u.n.o. 

VIII. All bolts are BS3692, grade 8.8 ordinary carbon steel bolts. None of which are external/exposed. Anything that could be considered external/exposed is galvanised.

IX. All bolt holes to be bolt diameter +2mm. Minimum edge distance for bolts to be 1.4xD and minimum spacing to be 2.0xD (where D = hole diameter). As per the submitted drawings. 

X. Internal steelwork was blast cleaned and received 1# coat of high-build epoxy zinc phosphate primer, dry film thickness 80 microns. The exposed internal steelwork has an alkyd finish applied, min thickness of 60 microns. Steel in exposed/external conditions to be hot-dipped galvanised to BS EN ISO 1461.

XI. Fire protection has been provided in accordance with the architect's details. 

(b) the particular physical features of the building that justify its designation as a listed building; and

I. The Old Manor House is a detached Grade II* listed property dating back to 1632 with distinctive flint elevations, stone mullion windows and tall gables. The property has an original Jacobean staircase across the three floors.

II. The property is also designated as star (*)  listed building on account of the visits made by Sir Winston Churchill and King George V whilst planning the D-Day Landings at the house during World War II.

(c) the building’s setting.
Unless the proposed works only affect the interior of the building, Design and Access Statements accompanying applications for listed building consent must also explain how issues relating to access to the building have been dealt with.
I. The works completed only affect the interior of the building.


