WALLS & ROOF
Rectangular wall structure – wood, 44mm thickness
Roof – Flat with EPDM rubber covering
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WINDOWS (PJO7) x 3
1530x340
Type: Fixed window with an integrated ventilation grate.
Material: Constructed from high-quality laminated solid timber to prevent warping and ensure durability.
Glazing: Fitted with 24mm HR++ double glazing (4 mm glass + 16 mm argon gas filled + 4 mm glass).

DOOR (PE46) x1 Single
1800x770
Laminated Timber: To prevent warping and shrinking, the door frame and posts are constructed from layered (laminated) European spruce.
Double Glazing: The door features 24mm HR++ double glazing (4mm glass + 16mm argon gas + 4mm glass)

Finish – Painted wood – Pebble grey – RAL 7032 – to complement adjacent stone façade of house.
Window and door trims painted white.

