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This Pollution Prevention Plan has been prepared to protect groundwater, surface water and land from contamination arising from the storage and distribution operations of agrochemical products
The plan identifies pollution risks and details the measures that will be implemented to prevent accidental releases of agrochemicals, fuels and other potentially polluting substances.
[bookmark: site-activities]1. Site Activities
· Storage of packaged agrochemicals including pesticides, herbicides, fungicides and liquid fertilisers.
· Loading and unloading of delivery vehicles.

[bookmark: potential-pollution-risks]2. Potential Pollution Risks
The principal pollution risks are:
· Spillage of agrochemical products.
· Release of contaminated Firewater.
· Contaminated surface water runoff.
· Fuel and oil leaks from vehicles and plant.
[bookmark: construction-phase-controls]
3. Controls
· [bookmark: fuel-and-oil-storage]Primary containment consists of UN approved packaging
· Secondary containment consists of Bunded Warehouse and Yard
· [bookmark: X613e305e95335234af6fe6a75e148b18d151065]Tertiary containment consists of Drainage control procedure
· Internal Emergency Preparedness Plan – Emergency Procedures


4. Operational Pollution Prevention Measures
[bookmark: concrete-and-washout]Concrete and Washout
· Concrete washout shall be undertaken only in designated contained areas.
· No washout water shall be discharged to drains, ditches or ground.
[bookmark: building-construction]Bunding
· The store shall be fully bunded to 185% of peak capacity.
· Floors shall be impermeable and chemical resistant.
· The floor shall be free from drainage outlets connected directly to surface water or groundwater.
· [bookmark: secondary-containment]Liquid chemicals shall be stored within dedicated bunded areas.
[bookmark: drainage]Drainage
· Contaminated water will be contained within bunded areas by way of gate/shutter valves
· Any potentially contaminated water shall be contained and disposed of by an appropriately licensed contractor.
[bookmark: storage-management]Storage Management
· Agrochemicals shall be stored in accordance with the yellow code
· Regular compliance audits to be undertaken by BASIS
· Products shall remain in original labelled containers.
· Incompatible products shall be segregated.
· Damaged containers shall be isolated immediately within the quarantine area.
[bookmark: loading-and-unloading]Loading and Unloading
· Deliveries shall be undertaken on impermeable hard standing.
· Staff shall supervise loading and unloading operations.
· Spill response materials shall be available throughout the site

[bookmark: firewater-management]5. Firewater Management
· In the event of a fire, contaminated firefighting water shall be contained on site within the warehouse bunding and the 2500Ltr drainage tank located in the yard thereafter.
· Site drainage shut-off arrangements shall be implemented to prevent discharge of contaminated firewater.
· Emergency services shall be informed of the presence and nature of stored agrochemicals.


[bookmark: spill-response-procedure]6. Response Procedures
· [bookmark: spill-response]As stated in IEPP for site

[bookmark: staff-training]7. Staff Training
· All employees handling agrochemicals shall receive appropriate training.
· Refresher training shall be provided periodically.
· Emergency response procedures shall communicated and practiced.

8. Waste Management
· Hazardous waste shall be stored in secure designated areas.
· Waste transfer documentation shall be retained.

[bookmark: inspection-and-monitoring]9. Inspection and Monitoring
The Site Manager shall undertake:
· Weekly inspections of storage areas.
· Monthly inspections of bunds and containment systems.
· Regular checks of spill kits and emergency equipment.
· Annual review of the Pollution Prevention Plan.
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