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Application for Discharge of Conditions 3 & 4  of  Reserved Matters approval PL/2022/09425 
Land at Elm Grove, Drynham Lane, Trowbridge, Wiltshire, BA14 0PL

	No
	Wording 
	Information submitted for discharge 

	3
	No demolition, site clearance or development shall commence on Phase 2 identified on drawing number 1955 119 Rev D until an Arboricultural Method Statement (AMS) relevant for that phase prepared by an arboricultural consultant providing
comprehensive details of construction works in relation to trees has been submitted to, and approved in writing by, the Local Planning Authority. All works shall subsequently be carried out in strict accordance with the approved details. In particular, the method statement must provide the following o A specification for protective fencing to trees during both demolition and construction phases which complies with BS5837:2013 and a plan indicating the alignment of the protective fencing;
o A specification for scaffolding and ground protection within tree protection zones in accordance with British Standard 5837: 2013;
o A schedule of tree works conforming to British Standard 3998: 2010;
o Details of general arboricultural matters such as the area for storage of materials,
concrete mixing.
o Plans and particulars showing the siting of the service and piping infrastructure;
o A full specification for the construction of any arboriculturally sensitive structures and sections through them, including the installation of boundary treatment works, the
method of construction of the access driveway including details of the no-dig
specification and extent of the areas of the driveway to be constructed using a no-dig specification;
o Details of the works requiring arboricultural supervision to be carried out by the
developer’s arboricultural consultant, including details of the frequency of supervisory visits and procedure for notifying the Local Planning Authority of the findings of the
supervisory visits; and
o Details of all other activities, which have implications for trees on or adjacent to the site.
o In order that trees to be retained on-site are not damaged during the construction
works and to ensure that as far as possible the work is carried no demolition, site
clearance or development should commence on site until a pre-commencement site
meeting has been held, attended by the developer’s arboricultural consultant and the designated site foreman.
	D21 87 02 Phase 2 Complete Elm Grove AMS
D21 87 P2 Rev A Trowbridge 2 TPP A1 P 500

	4
	No demolition, site clearance or development shall commence on Phase 3 identified on drawing number 1955 119 Rev D until an Arboricultural Method Statement (AMS) relevant for that phase prepared by an arboricultural consultant providing
comprehensive details of construction works in relation to trees has been submitted to, and approved in writing by, the Local Planning Authority. All works shall subsequently be carried out in strict accordance with the approved details. In particular, the method statement must provide the following o A specification for protective fencing to trees during both demolition and construction phases which complies with BS5837:2013 and a plan indicating the alignment of the protective fencing;
o A specification for scaffolding and ground protection within tree protection zones in accordance with British Standard 5837: 2013;
o A schedule of tree works conforming to British Standard 3998: 2010;
o Details of general arboricultural matters such as the area for storage of materials,
concrete mixing.
o Plans and particulars showing the siting of the service and piping infrastructure;
o A full specification for the construction of any arboriculturally sensitive structures and sections through them, including the installation of boundary treatment works, the
method of construction of the access driveway including details of the no-dig
specification and extent of the areas of the driveway to be constructed using a no-dig specification;
o Details of the works requiring arboricultural supervision to be carried out by the
developer’s arboricultural consultant, including details of the frequency of supervisory visits and procedure for notifying the Local Planning Authority of the findings of the
supervisory visits; and
o Details of all other activities, which have implications for trees on or adjacent to the site.
o In order that trees to be retained on-site are not damaged during the construction
works and to ensure that as far as possible the work is carried no demolition, site
clearance or development should commence on site until a pre-commencement site
meeting has been held, attended by the developer’s arboricultural consultant and the designated site foreman.
	D21 87 P2 Rev A Trowbridge 2 TPP A1 P 500
D21 87 P3 Rev A Trowbridge Phase 3 TPP A1 P 500





Notes on compliance with Conditions 3 & 4:

o A specification for protective fencing to trees during both demolition and construction phases which complies with BS5837:2013 and a plan indicating the alignment of the protective fencing; Included in the TPPs
o A specification for scaffolding and ground protection within tree protection zones in accordance with British Standard 5837: 2013; we are not proposing any scaffolding  within RPAs of retained trees and hedges
o A schedule of tree works conforming to British Standard 3998: 2010; We are not undertaking any specific tree surgery within the scope of BS 3998, we are cutting back various lengths of hedges where needed – indicated in orange on the TPPs
o Details of general arboricultural matters such as the area for storage of materials, concrete mixing; The AMS confirms that there will be no impact on retained trees or hedges
o Plans and particulars showing the siting of the service and piping infrastructure; The AMS/ TPP is based on the detailed engineering and suggested that plot and strategic infrastructure is located below the roads, drives and paths
o A full specification for the construction of any arboriculturally sensitive structures and sections through them, including the installation of boundary treatment works. The AMS states the method of construction of the access driveway including details of the no-dig. 
specification and extent of the areas of the driveway to be constructed using a no-dig specification; We are not using any specialist or ‘No-dig’ surfaces
o Details of the works requiring arboricultural supervision to be carried out by the developer’s arboricultural consultant, including details of the frequency of supervisory visits and procedure for notifying the Local Planning Authority of the findings of the
supervisory visits; and The requirement to regularly visit site during construction is included in the AMS
o Details of all other activities, which have implications for trees on or adjacent to the site. N/A
o In order that trees to be retained on-site are not damaged during the construction works and to ensure that as far as possible the work is carried no demolition, site clearance or development should commence on site until a pre-commencement site meeting has been held, attended by the developer’s arboricultural consultant and the designated site foreman. Included in the AMS
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