Garage Plot 1 Forest Fields East Grafton 
Notes re materials

External cladding
This is the description of the cladding taken from Barlows Timber Woodyard website.  
Sawn treated softwood.
175mm feather edge cladding treated
The 175mm sawn treated cladding has two boards cut from a 32mm x 175mm timber, then treated for longer life.
Colour light brown.
This is the approved material used for the two recently constructed garages on the site. It is proposed to use the same material from the same supplier.

Roof tiles
Plain clay tiles exactly as approved for the adjacent house roof.

