We would add a soakaway from designed crates to the garden @ 5 metres away to take the rain from hardscaping. Route new roof gutter and existing to reduce overflowing the sewage system. This will allow the surface road drainage to be less congested with new supplies.
