Soakaway design and construction description;
* Type: A below-ground modular plastic crate soakaway.
* Location: Positioned within the property’s garden/land, at least 5m from property.
* Purpose: To receive and infiltrate surface water collected from the extension roof gutters/downpipes.
* Construction: The soakaway will be excavated to the required size and depth, with the dimensions determined from the drainage calculations and percolation test results. The excavation will be lined with a suitable geotextile membrane, with modular plastic soakaway crates installed within the excavation. The crates will be surrounded/wrapped with geotextile and the excavation backfilled with suitable excavated/imported material.
* Inlet: Surface water from the extension will be conveyed via underground drainage pipework from the downpipes to the soakaway. Pipework will be laid to an appropriate fall.
* Access/maintenance: Our responsibility.
* Construction responsibility: The soakaway and associated drainage will be constructed by Daniel Jordan (Plumber), in accordance with the manufacturer’s installation requirements.
* Testing: VP Tests completed and approved.
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