We have performed the test as outlined below over 2 days. A few photos attached. 

Test 1 -  VP = 40.29
Test 2- VP = 53.82
Test 3 - VP = 19.45

All well within the expected parameters. 

With regards to the cross section drawing we are still at the loose end, we have contacted multiple builders to see if they have ever had anyone have to do this and if they have a contact to assist and come out with nothing! I do not know where to go from here. Something a small as this is really risking the planning to lapse and us having to start again and being even more out of pocket. As building would be signing this off along with the footings before cover it, would that not suffice? 
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