ADDENDUM STATEMENT   in connection with location of external oil fired boiler for central heating and hot water at 289 Ablington for Messer Rawlins 
The location of the boiler and oil tank has been submitted, further information has been requested. A plumbing contractor has not selected the exact boiler at this time but external appearance will be as submitted.
The property has a hot water tank located in the kitchen serving the kitchen and bathroom on the ground floor, this has immersion heater.
The hot water tank will be changed to a pressurized insulated indirect cylinder with stand by immersion heater , flow and returns will run from the boiler to the tank possibly 22mm dia pipe with insulation.
[bookmark: _GoBack]Existing feeds off the cylinder will run to existing fittings and connect through a ball fix joint
Central heating will be based on a drop feed system with pipes [possibly 15mm dia] being above the first floor with drops to the ground floor. 
Radiators will be convector panel radiators Btu rating to suit the room positions subject to space and fitted with thermostatic valves.
System will be filled tested and run.

 


