DAS for Emergency Repair to front wall of 43-45 London Road
· Introduction:
This DAS is related to the need to make safe the east side front boundary wall of 43-45 London Road.  The wall is bowing heavily, the gate pillar leaning and the council have had a complaint it may not be safe.  
· Description of the Existing Site and Proposal:
2. Existing Site: The boundary wall to London Road for 43-45 London Road including the gate pillar containing the Albert of Albert Cottages.
2. Proposed Repair: tTo dismantle the wall, make safe the footings and rebuild using the original materials
· Design Principles and Concepts:
3. Urgency and Justification: the repair is needed because the wall is unsafe
3. Suitability: the repair will replicate the original wall using the original materials in the order they were dismantled.
· Access:
4. Approach: Access to the property will be maintained and unchanged.
4. Standards: Outline any relevant access standards or guidance that will be followed for the repair work. 
· Compliance with Policies:
5. The repair takes place following consultations with the council representatives

· Conclusion:  The repair is needed to make the wall safe and to ensure its long term future as part of the frontage of the house.  Particular reference is made to the pillars in the listing.  A collapse of the wall would potentially see the pillar lost.

