. I can confirm the following:
1. Street lighting column protection:
A 360° heavy duty lamp post protector will be installed to guard against collision damage. Specification to be high-grade steel with hot-dip galvanised finish, height: 600mm, outer diameter: 350mm, tube diameter: 48mm, bolt-down installation with pre-drilled base plate holes for surface fixing
2. Car parking spaces for Plot 35A dimensions:
I confirm the two parking spaces for Plot 35A are 2.4m x 4.8m.
3. Double garage for Plot 35B dimensions:
The double garage has been enlarged and now measures 6.0m x 4.8m (internal dimensions).
4. Access rights:
The applicant has confirmed there are access rights over the shared driveway.
5. Yellow hatched area - parking restriction:
I confirm the area highlighted yellow (at the top of the shared drive within Plot 35A ownership) is for access only and will not be used for parking.
Please find attached revised drawing 25016/P004 Rev A - Proposed Site Plan showing:
1. Car parking spaces for Plot 35A dimensioned at 4.8m x 2.4m
1. Lamp post protector added
1. Double garage enlarged to 6.0m x 4.8m
1. Note added: "Area at top of shared drive within plot 35A not to be used for parking"

