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Issue 1
For
New Dwelling, Two Bedroom Bungalow with Double Carport
At

Summerleaze Lodge 10 Beanacre Melksham SN12 7PT
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Proposal

To seek Change of Use of part of an existing paddock to domestic. To then build a two bedroom bungalow with an attached double carport.
The Site
The site is generally flat at 41m above average sea level. The site is shown not to be  in a flood zone. 
Environment Agency Flood Map
The site has been outlined in red.
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Flood Zones 2 & 3

Design against flood.
Although the site is not in a Flood Zone, after exceptional rainfall or storms surface water has been seen in the paddock. To help mitigate the loss of permeable surface now occupied by the building. Firstly, surface water from the roof will be collected in water butts for garden use. Then the overflow will be directed to an underground rainwater harvesting system. The collected water to be used for toilet flushing, laundry, garden irrigation etc. The main drive and parking to be permeable gravel to the vehicle entrance. The patio and paths again will be of a permeable surface.  The additional tree planting along the boundary will also have a demand for rainwater. The floor level of the house will be positioned 300mm above ground level rather than the normal 150mm.  
