1. The proposal will connect to the existing drainage system.
1. Drawings updated from Preliminary to Planning.
1. The height from FFL of the rooflights on the side elevations is 1100mm. This is to allow for fire egress, to comply with Building Regulations Part B. On the front elevations, the rooflights are 1390mm above FFL as fire egress is provided by the side elevation rooflight of Bedroom 3 and is not required for the bathroom.
1. Drawings updated to show carport post moved and cycle storage provision.
1. Updated parking allocation plan provided. 

