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Listed materials information.



Proposed Opposite-Handed Car Barn at:

Midge Hall
Coped Hall
Royal Wootton Basett
SN4 8ER





On behalf of:
Julian Hayward



Prepared by:
Equestrian Blueprint
enquiries@equestrianblueprint.co.uk
https://equestrianblueprint.co.uk/
May 2026


Garden boundary wall.

Existing historic boundary wall constructed in traditional handmade red/orange clay brickwork laid in lime mortar, incorporating varied tonal colouring and weathered historic fabric characteristic of vernacular estate walling. Bricks are circa 60mmx100mmx215mm.

Bricks for proposed wall to stop-up the existing access in the garden wall, and the plinth for the proposed garage. This is a sample that are being cleaned up for reuse
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Clay tiles to be used on the new garage.

Reclaimed clay plain roof tiles with traditional weathered finish and varied natural colouring
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Double Field Gate

The gate will be pressure treated and have a mid-brown finish.
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