Heritage Statement – window repair and paint removal

These works are essential to repair the damage caused to a stone window and paintwork on the front elevation of the building.  These works are essential to maintain the property in good repair following this damage.  The removal of the flaky paintwork will assist in maintaining the brickwork in good order, avoiding brick damage in future from future rainwater/ice getting under any paint.  
We will be employing the services of a highly experienced stonemason who has local knowledge of the stonework involved.  Given the age of the building it may not be possible to find an exact colour match of the stone and this is one reason we are employing this individual in the selected company; with his local and stonework knowledge and experience, he has the best chance to find a good match. 
Aside from colour match challenge (which there is no option to avoid) we anticipate no detrimental effect on the character or structure of this building.   These works are necessary to restore the damaged window frame and avoid further deterioration, and remove flaky paintwork which poses a risk to the brickwork underneath. 
Regarding access, no neighbouring properties will be significantly affected by these works, which are anticipated to be completed within one week from commencement.  Scaffolding will have to be used to remove paintwork at higher levels, however this will be limited to the width of the building and not extend any further.  There is usually plenty of parking available in the car park fronting the building such that no neighbours should be inconvenienced during the works.
