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Application for Discharge of Conditions 8, 9, 26, 32 & 35 of  planning application 19/11459/OUT at Land at Elm Grove, Drynham Lane, Trowbridge, Wiltshire, BA14 0PL

	No
	Condition Wording
	Submitted Plans/Notes
	Applicable To

	8
	Notwithstanding the Parameters Levels Plan, no development shall commence in any phase until plans showing finished floor levels (FFL) and threshold levels for the phase have been submitted to and approved in writing with the Local Planning Authority. These plans should set minimum FFLs at the 1 in 100 year plus climate change level with a 300mm freeboard OR the 1 in 1000 year flood level with downstream culvert blockage. The development shall be caried out in accordance with the approved details.
	
1960_2601_C1 EXTERNAL WORKS LAYOUT
1960_2602_C1 EXTERNAL WORKS LAYOUT
1960_2603_C1 EXTERNAL WORKS LAYOUT
1960_2604_C1 EXTERNAL WORKS LAYOUT
1960_2605_C1 EXTERNAL WORKS LAYOUT
1960_2606_C1 EXTERNAL WORKS LAYOUT
1960_3601-C2_EXTERNALS WORKS LAYOUT SHEET 1
1960_3602-C2_EXTERNALS WORKS LAYOUT SHEET 2
1960_3603-C2_EXTERNALS WORKS LAYOUT SHEET 3
1960_3604-C1_EXTERNALS WORKS LAYOUT SHEET 4


Note that :1960w003 Elm Grove, Trowbridge JRC Flood Risk Assessment Addendum P5, approved as part of PL/2024/09649 provides confirmation of compliance with the requirement to set minimum FFLs at the 1 in 100 year plus climate change level with a 300mm freeboard OR the 1 in 1000 year flood level with downstream culvert blockage.


	Phases 2-4 as depicted on drawing 1119 approved under Condition 4. This provides the remaining information to discharge condition 8 following an earlier partial discharge for Phase 1.

	9
	No development shall commence until a scheme for discharge of surface water from the site, including sustainable drainage systems, exceedance flow routes and all third party approvals, has been submitted to and approved in writing by the Local Planning Authority/Lead Local Flood Authority. This scheme shall include a programme of phasing, implementation and maintenance for the lifetime of the development. The development shall be caried out in accordance with the approved details.
	1960_010_C_SMP_P2 SuDS Maintenance & Management Plan
1955_1114E_Trowbridge_Enclosures Plan
1960_2141-TA1_GULLY CATCHMENT AREA PLAN-SHEET 1
1960_2142-TA1_GULLY CATCHMENT AREA PLAN-SHEET 2
1960_2143-TA1_GULLY CATCHMENT AREA PLAN-SHEET 3
1960_2144-TA1_GULLY CATCHMENT AREA PLAN-SHEET 4
1960_2145-TA1_GULLY CATCHMENT AREA PLAN-SHEET 5
1960_2146-TA1_GULLY CATCHMENT AREA PLAN-SHEET 6
1960_2501_C1_DRAINAGE LAYOUT
1960_2502_C1_DRAINAGE LAYOUT
1960_2503_C1_DRAINAGE LAYOUT
1960_2504_C1_DRAINAGE LAYOUT
1960_2505_C1_DRAINAGE LAYOUT
1960_2506_C1_DRAINAGE LAYOUT
1960_2511_TA4 S104 DRAINAGE LAYOUT
1960_2521-TA1_SURFACE WATER DRAINAGE LONGSECTIONS-SHEET 1
1960_2522-TA1_SURFACE WATER DRAINAGE LONGSECTIONS-SHEET 2
1960_2540-TA2_SURFACE WATER DRAINAGE MANHOLE SCHEDULES
1960_2571_C1 PRIVATE DRAINAGE CONSTRUCTION DETAILS
1960_2572_C1 PRIVATE DRAINAGE CONSTRUCTION DETAILS
1960_2573_C1 PRIVATE DRAINAGE CONSTRUCTION DETAILS
1960_2593-TA1_OWC DITCH CULVERT AND IMPROVEMENT WORKS LAYOUT
1960_2594-TA2_OWC DITCH CULVERT AND IMPROVEMENT WORKS SECTIONS
1960_2594-TA3_OWC DITCH CULVERT AND IMPROVEMENT WORKS SECTIONS
1960_2595-TA1_WETLAND BASIN 2 SECTION
1960_2596-TA1_WETLAND BASIN 3
1960_2597-TA1_WETLAND BASIN 3 SECTION - SHEET 1
1960_2598-TA1_WETLAND BASIN 3 SECTION - SHEET 2
1960_2721-TA1_HIGHWAYS SPECIFICATION LAYOUT-SHEET 1
1960_2722-TA1_HIGHWAYS SPECIFICATION LAYOUT-SHEET 2
1960_2723-TA1_HIGHWAYS SPECIFICATION LAYOUT-SHEET 3
1960_2724-TA1_HIGHWAYS SPECIFICATION LAYOUT-SHEET 4
1960_2725-TA1_HIGHWAYS SPECIFICATION LAYOUT-SHEET 5
1960_2726-TA1_HIGHWAYS SPECIFICATION LAYOUT-SHEET 6
1960_3501_TA2_DRAINAGE LAYOUT SHEET 1
1960_3502_TA2_DRAINAGE LAYOUT SHEET 2
1960_3503_TA2_DRAINAGE LAYOUT SHEET 3
1960_3721-TA1_HIGHWAY SPECIFICATION LAYOUT
1960_3722-TA1_HIGHWAY SPECIFICATION LAYOUT
1960_3723-TA1_HIGHWAY SPECIFICATION LAYOUT
1960_3724-TA1_HIGHWAY SPECIFICATION LAYOUT
1960_3725-TA1_HIGHWAY SPECIFICATION LAYOUT
1960_3726-TA1_HIGHWAY SPECIFICATION LAYOUT

	Phases 2-4 as depicted on drawing 1119 approved under Condition 4. This provides the remaining information to discharge condition 9 following an earlier partial discharge for Phase 1.

	26
	Within 3 months of first occupation of the development hereby approved a full travel plan shall be submitted based on the framework travel plan included in the planning application. The full travel plan when approved shall be implemented including the appointment of a travel plan co-ordinator for three years from the date of first appointment.
	Residential Travel Plan (10027) Issue 2 January 2026 
	This information is relevant for all phases. 

	32
	No development shall commence in any phase of the development hereby approved until a scheme of hard and soft landscaping for the phase has been submitted to and approved in writing by the Local Planning Authority, the details of which shall include:

• location and current canopy spread of all existing trees and hedgerows on the land
• full details of any to be retained, together with measures for their protection during development
• a detailed planting specification showing all plant species, supply and planting sizes and planting densities, together with details of how grassland habitats will be established
• finished levels and contours
• means of enclosure
• car park layouts
• other vehicle and pedestrian access and circulation areas
• all hard and soft surfacing materials
• minor artefacts and structures (e.g. furniture, play equipment, refuse and other storage units, signs, lighting etc)
• proposed and existing functional services above and below ground (e.g. drainage, power, communications, cables, pipelines etc indicating lines, manholes, supports etc
• retained historic landscape features and proposed restoration, where relevantAll trees tree(s) shall be planted in accordance with BS3936 (Parts 1 and 4), BS4043 and BS4428
	P22-1514_EN_007A Detailed Soft On-plot Landscape Proposals (197 units)
(detailed planting specification showing all plant species, supply and planting sizes and planting densities)

Arboricultural Report (August 2024) and Addendum (6/11/24) 
(Showing location and current canopy spread of all existing trees and hedgerows on the land and full details of any to be retained, together with measures for their protection during development)
 
1960_2721-TA1_HIGHWAYS SPECIFICATION LAYOUT-SHEET 1
1960_2722-TA1_HIGHWAYS SPECIFICATION LAYOUT-SHEET 2
1960_2723-TA1_HIGHWAYS SPECIFICATION LAYOUT-SHEET 3
1960_2724-TA1_HIGHWAYS SPECIFICATION LAYOUT-SHEET 4
1960_2725-TA1_HIGHWAYS SPECIFICATION LAYOUT-SHEET 5
1960_2726-TA1_HIGHWAYS SPECIFICATION LAYOUT-SHEET 6
1960_3721-TA1_HIGHWAY SPECIFICATION LAYOUT
1960_3722-TA1_HIGHWAY SPECIFICATION LAYOUT
1960_3723-TA1_HIGHWAY SPECIFICATION LAYOUT
1960_3724-TA1_HIGHWAY SPECIFICATION LAYOUT
1960_3725-TA1_HIGHWAY SPECIFICATION LAYOUT

1960_3726-TA1_HIGHWAY SPECIFICATION LAYOUT (Showing finished levels and contours, all hard surfacing materials and other vehicle and pedestrian access and circulation areas)

13.  1960_2506_C1_DRAINAGE LAYOUT
1960_2505_C1_DRAINAGE LAYOUT
1960_2504_C1_DRAINAGE LAYOUT
1960_2503_C1_DRAINAGE LAYOUT
1960_2502_C1_DRAINAGE LAYOUT
1960_2501_C1_DRAINAGE LAYOUT
1960_3503_TA2_DRAINAGE LAYOUT SHEET 3
1960_3502_TA2_DRAINAGE LAYOUT SHEET 2
1960_3501_TA2_DRAINAGE LAYOUT SHEET 1
 (Showing drainage, pipelines etc indicating lines, manholes, supports etc)

Noting the following are already approved as part of RM Plans: 
General Landscape Specification Rev G
P22-1514_EN_001F Landscape Masterplan; 
P22-1514_EN_002F-Sht3 Detailed POS Landscape Proposals; P22-1514_EN_002F-Sht4 Detailed POS Landscape Proposals; P22-1514_EN_004B_Sht1 On-plot Tree Landscape Proposals 

	Phases 2-4 as depicted on drawing 1119 approved under Condition 4. This provides the remaining information to discharge condition 32 following an earlier partial discharge for Phase 1.

	35
	No external lighting shall be installed on site until plans showing:

• the type of light appliance,
• the height and position of fitting,
• illumination levels and
• light spillage
have been submitted to and approved in writing by the Local Planning Authority. The Plans will be in accordance with the appropriate Environmental Zone standards set out by the Institute of Lighting Engineers in their publication GN01:2011, ‘Guidance for the Reduction of Obtrusive Light’ (ILP, 2011), and Guidance Note GN08-18 “Bats and artificial Lighting in the UK” published by the Bat Conservation Trust and Institution of Lighting Engineers.

Where light spill has the potential to impact core bat habitat, the lighting impact assessment of the reserved matters applications(s) must meet the requirements of section 8.3 of the Trowbridge Bat Mitigation Strategy in terms of the methodology for predicting post-development lighting conditions; maintenance of illuminance zones A, B and C, and; lighting design solutions.
The approved lighting shall be installed and maintained in accordance with the approved details and no additional external lighting shall be installed.

This condition will be discharged when a post-development lighting survey conducted in accordance with section 8.3.4 of the Trowbridge Bat Mitigation Strategy has been submitted to the Local Planning Authority demonstrating compliance with the approved lighting plans, having implemented and retested any necessary remedial measures.
	P24896-DRG-S38-20-p01
P24896-DRG-S38-21-p01
P24896-DRG-S38-22-p01
P24896-DRG-S38-23-p01
P24896-DRG-S38-24-p01
P24896-DRG-S38-25-p01
P24896-DRG-S38-Ph3-30-1-p01 (Maint)
P24896-DRG-S38-Ph3-30-2-p01 (Maint)
P24896-DRG-S38-Ph3-31-1-p01 (MF1)
P24896-DRG-S38-Ph3-31-2-p01 (MF1)
P24896-DRG-S38-Ph3-32-1-p01 (Eng)
P24896-DRG-S38-Ph3-32-2-p01 (Eng)
P24896-LRA-05 (S38-Ph2 MF0.87)
P24896-LRA-06 (S38-Ph2 MF1)
P24896-LRA-Ph3-MF1
P24896-LRA-Ph3-MF087
	Phases 2-4 as depicted on drawing 1119 approved under Condition 4. This provides the remaining information to discharge condition 35 following an earlier partial discharge for Phase 1.
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